City Of Shelley Design Loads Table R301.2(1)

* Seismic Design Category C or D
* Ground Snow Load 42+
* Wind Load 90 MPH
* Frost Depth 30 Inches
* Ice Barrier Underlayment Required Yes
* Weathering Severe
* Winter Design Temp Negative 4
* Air Freezing Index 2000
* Mean Annual Temp 45 °F
* Termite Slight / Moderate